Device Rev 3, DD Rev 1
   150 response_code                    ENUMERATED       1
   151 device_status                    BIT_ENUMERATED   1
   152 comm_status                      BIT_ENUMERATED   1
   153 manufacturer_id                  ENUMERATED       1
   154 device_type                      ENUMERATED       1
   155 request_preambles                UNSIGNED         1
   156 universal_revision               UNSIGNED         1
   157 transmitter_revision             UNSIGNED         1
   158 software_revision                UNSIGNED         1
   159 hardware_revision                UNSIGNED         1
   160 device_flags                     BIT_ENUMERATED   1
   161 device_id                        UNSIGNED         3
   162 polling_address                  UNSIGNED         1
   163 tag                              PACKED_ASCII     8
   164 message                          PACKED_ASCII    32
   165 descriptor                       PACKED_ASCII    16
   166 date                             DATE             3
   167 write_protect                    ENUMERATED       1
   168 private_label_distributor        ENUMERATED       1
   169 final_assembly_number            UNSIGNED         3
   171 physical_signaling_code          ENUMERATED       1
   233 percentRange                     FLOAT            4
   234 upperRange_value                 FLOAT            4
   235 lowerRange_value                 FLOAT            4
   236 loop_alarm_code                  ENUMERATED       1
   237 loopCurrent                      FLOAT            4
  2028 material_code                    ENUMERATED       1
  2043 device_variable_classification_codes ENUMERATED       1
  2045 write_device_variable_codes      ENUMERATED       1
  2047 trim_point_codes                 ENUMERATED       1
  2049 device_variable_family_codes     ENUMERATED       1
  2051 capture_mode_codes               ENUMERATED       1
  2052 process_data_status              ENUMERATED       1
  2053 limit_status                     ENUMERATED       1
  2246 device_variable_code_codes       ENUMERATED       1
  2311 units_code_temperature           ENUMERATED       1
  2427 dev_var_property_codes           BIT_ENUMERATED   1
  2440 squawk_control                   ENUMERATED       1
  2732 std_device_family_status         BIT_ENUMERATED   1
  4048 primary_variable_code            INDEX            1
  4049 secondary_variable_code          INDEX            1
  4139 device_specific_status_0         BIT_ENUMERATED   1
  4140 device_specific_status_1         BIT_ENUMERATED   1
  4141 device_specific_status_2         BIT_ENUMERATED   1
  4142 device_specific_status_3         BIT_ENUMERATED   1
  4143 device_specific_status_4         BIT_ENUMERATED   1
  4144 device_specific_status_5         BIT_ENUMERATED   1
  4167 device_variable_code             INDEX            1
  8068 transfer_function                ENUMERATED       1
 16384 standardized_status_00           BIT_ENUMERATED   1
 16385 temperatureValue                 FLOAT            4
 16386 temperatureUnits                 ENUMERATED       1
 16387 temperatureFamily                ENUMERATED       1
 16388 temperaturePDQ                   ENUMERATED       1
 16389 temperatureLS                    ENUMERATED       1
 16390 temperatureStatus                BIT_ENUMERATED   1
 16391 temperatureUSL                   FLOAT            4
 16392 temperatureLSL                   FLOAT            4
 16393 temperatureMinimumSpan           FLOAT            4
 16394 temperatureDampingValue          FLOAT            4
 16395 temperatureUpdatePeriod          TIME_VALUE       4
 16396 temperatureSimulated             ENUMERATED       1
 16397 temperatureSerialNumber          UNSIGNED         3
 16398 temperatureProperties            BIT_ENUMERATED   1
 16399 temperatureClassification        ENUMERATED       1
 16401 fixedSensor                      ENUMERATED       1
 16402 sensorMalfunction                ENUMERATED       1
 16403 sensorType                       ENUMERATED       1
 16404 sourceType                       ENUMERATED       1
 16405 deviceType                       ENUMERATED       1
 16406 cjStatus                         ENUMERATED       1
 16407 peak_min_user_pv                 FLOAT            4
 16408 peak_max_user_pv                 FLOAT            4
 16409 peak_min_factory_pv              FLOAT            4
 16410 peak_max_factory_pv              FLOAT            4
 16411 pinCode                          UNSIGNED         4
 16412 dummyByte                        UNSIGNED         1
 16413 dummyByte2                       UNSIGNED         2
 16414 dummyByte3                       UNSIGNED         3
 16415 dummyByte4                       UNSIGNED         4
 16416 firmware_CRC                     UNSIGNED         2
 16417 firmware_metrolog_CRC            UNSIGNED         2
 16418 adjustRawSensor                  FLOAT            4
 16419 adjustEtalon                     FLOAT            4
 16420 coefAdjust_zero                  FLOAT            4
 16421 coefAdjust_span                  FLOAT            4
 16422 pvSimulation                     FLOAT            4
 16423 std_standardized_status_0_codess BIT_ENUMERATED   1
 16470 GaugeConditionalLRedBandValueVar FLOAT            4
 16472 GaugeConditionalYellowBandValueVar FLOAT            4
 16473 GaugeConditionalGreenBandValueVar FLOAT            4
 16474 GaugeConditionalHYellowBandValueVar FLOAT            4
 16475 GaugeConditionalRedBandValueVar  FLOAT            4
