Device Rev 1, DD Rev 1
   150 response_code                    ENUMERATED       1
   151 device_status                    BIT_ENUMERATED   1
   152 comm_status                      BIT_ENUMERATED   1
   153 manufacturer_id                  ENUMERATED       2
   154 device_type                      ENUMERATED       2
   155 request_preambles                UNSIGNED         1
   156 universal_revision               UNSIGNED         1
   157 transmitter_revision             UNSIGNED         1
   158 software_revision                UNSIGNED         1
   159 hardware_revision                UNSIGNED         1
   160 device_flags                     BIT_ENUMERATED   1
   161 device_id                        UNSIGNED         3
   162 polling_address                  UNSIGNED         1
   163 tag                              PACKED_ASCII     8
   164 message                          PACKED_ASCII    32
   165 descriptor                       PACKED_ASCII    16
   166 date                             DATE             3
   167 write_protect                    ENUMERATED       1
   168 private_label_distributor        ENUMERATED       2
   169 final_assembly_number            UNSIGNED         3
   171 physical_signaling_code          ENUMERATED       1
   206 max_num_device_variables         UNSIGNED         1
   207 config_change_counter            UNSIGNED         2
   210 longTag                          ASCII           32
   225 device_variable_code_1           INDEX            1
   226 device_variable_code_2           INDEX            1
   227 device_variable_code_3           INDEX            1
   228 device_variable_code_4           INDEX            1
   231 loop_flags                       BIT_ENUMERATED   1
   233 percentRange                     FLOAT            4
   234 upperRange_value                 FLOAT            4
   235 lowerRange_value                 FLOAT            4
   236 loop_alarm_code                  ENUMERATED       1
   237 loopCurrent                      FLOAT            4
   254 time_stamp                       TIME_VALUE       4
   255 device_profile                   ENUMERATED       1
   256 device_variable_code_5           INDEX            1
   257 device_variable_code_6           INDEX            1
   258 device_variable_code_7           INDEX            1
   259 device_variable_code_8           INDEX            1
   260 standardized_status_0            BIT_ENUMERATED   1
  2028 material_code                    ENUMERATED       1
  2043 device_variable_classification_codes ENUMERATED       1
  2045 write_device_variable_codes      ENUMERATED       1
  2047 trim_point_codes                 ENUMERATED       1
  2049 device_variable_family_codes     ENUMERATED       1
  2051 capture_mode_codes               ENUMERATED       1
  2052 process_data_status              ENUMERATED       1
  2053 limit_status                     ENUMERATED       1
  2055 extended_fld_device_status       BIT_ENUMERATED   1
  2056 loop_current_mode                ENUMERATED       1
  2246 device_variable_code_codes       ENUMERATED       1
  2311 units_code_temperature           ENUMERATED       1
  2427 dev_var_property_codes           BIT_ENUMERATED   1
  2440 squawk_control                   ENUMERATED       1
  2732 std_device_family_status         BIT_ENUMERATED   1
  4048 primary_variable_code            INDEX            1
  4049 secondary_variable_code          INDEX            1
  4066 response_preambles               UNSIGNED         1
  4139 device_specific_status_0         BIT_ENUMERATED   1
  4140 device_specific_status_1         BIT_ENUMERATED   1
  4141 device_specific_status_2         BIT_ENUMERATED   1
  4142 device_specific_status_3         BIT_ENUMERATED   1
  4143 device_specific_status_4         BIT_ENUMERATED   1
  4144 device_specific_status_5         BIT_ENUMERATED   1
  4167 device_variable_code             INDEX            1
  8068 transfer_function                ENUMERATED       1
 16384 temperatureValue                 FLOAT            4
 16385 temperatureUnits                 ENUMERATED       1
 16386 temperatureFamily                ENUMERATED       1
 16387 temperaturePDQ                   ENUMERATED       1
 16388 temperatureLS                    ENUMERATED       1
 16389 temperatureStatus                BIT_ENUMERATED   1
 16390 temperatureUSL                   FLOAT            4
 16391 temperatureLSL                   FLOAT            4
 16392 temperatureMinimumSpan           FLOAT            4
 16393 temperatureDampingValue          FLOAT            4
 16394 temperatureUpdatePeriod          TIME_VALUE       4
 16395 temperatureSimulated             ENUMERATED       1
 16396 temperatureSerialNumber          UNSIGNED         3
 16397 temperatureProperties            BIT_ENUMERATED   1
 16398 temperatureClassification        ENUMERATED       1
 16400 fixedSensor                      ENUMERATED       1
 16401 sensorMalfunction                ENUMERATED       1
 16402 sensorType                       ENUMERATED       1
 16403 sourceType                       ENUMERATED       1
 16404 deviceType                       ENUMERATED       1
 16405 outputHighValue                  FLOAT            4
 16406 pinCode                          UNSIGNED         4
 16407 dummyByte                        UNSIGNED         1
 16408 dummyByte2                       UNSIGNED         2
 16409 dummyByte3                       UNSIGNED         3
 16410 dummyByte4                       UNSIGNED         4
 16411 firmware_CRC                     UNSIGNED         2
 16412 firmware_metrolog_CRC            UNSIGNED         2
 16413 adjustRawSensor                  FLOAT            4
 16414 adjustEtalon                     FLOAT            4
 16415 coefAdjust_zero                  FLOAT            4
 16416 coefAdjust_span                  FLOAT            4
 16417 sensorCalcType                   ENUMERATED       1
 16418 kvdA                             DOUBLE           8
 16419 kvdB                             DOUBLE           8
 16420 kvdR0                            DOUBLE           8
 16467 GaugeConditionalLRedBandValueVar FLOAT            4
 16469 GaugeConditionalYellowBandValueVar FLOAT            4
 16470 GaugeConditionalGreenBandValueVar FLOAT            4
 16471 GaugeConditionalHYellowBandValueVar FLOAT            4
 16472 GaugeConditionalRedBandValueVar  FLOAT            4
